|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **IBM Contacts:**  **Writer/Requester:**  **EC Management:** | SPEC Owner: Michal Malostik (email: [michal.malostik@sk.ibm.com](mailto:michal.malostik@sk.ibm.com))  011 421 908 546 586 - to call from US  00 421 908 546 586 - to call from Mexico   |  |  | | --- | --- | | Backup: Marek Mikulasovic (email: [marek.mikulasovic@sk.ibm.com](mailto:marek.mikulasovic@sk.ibm.com))  011 421 907 377 241 - to call from US  00 421 907 377 241 - to call from Mexico |  |   Backup: Sharon Norton (507) 253-2150 (email: [sharonn@us.ibm.com](mailto:sharonn@us.ibm.com))  Ryan Achilles (email: [achilles@us.ibm.com](mailto:achilles@us.ibm.com))  EC creator: [peter.holenda@sk.ibm.com](mailto:peter.holenda@sk.ibm.com)  EC creator’s backup: [Tomas.Bvoc1@ibm.com](mailto:Tomas.Bvoc1@ibm.com) | | |
| **EC Level:** | P45258 | | |
| **.ZIP Package Contents:**  **ZIP File Location:**  **Form Number** | 03KG302.doc  I1199149.pdf  CoO Barcode.pdf  03KG302A.zip  GI11-9914-09 | | Print Instructions and Specification (this file)  Camera Ready Copy (CRC) (Covers and Body Text)  Country of Origin (CoO)  **http://public.dhe.ibm.com/systems/power/docs/hw/OMS/** |
| **Component:** | Hardcopy Manual | | |
| **Cover:** | Stock:  Color: | 80lb opaque white (or IBM approved equivalent)  2-color (black and Pantone 2718 blue) | |
| **Body Text:** | Stock:  Color:  Prints:  Page Count: | 20lb opaque white (or IBM approved equivalent)  6-color: Black, Pantone 032 Red, Pantone 108 Yellow, Pantone 2718 Blue, Pantone 1525 C Orange, Green  2 sides (duplex)  62 | |
| **Binding:** | Saddle Stitch | | |
| **Trim size:** | 8.5-in. by 11.0-in. | | |
| **Orientation:** | Portrait | | |
| **Collation:** | See the .PDF for a representative sample. | | |
| **Additional Instructions:**   1. Outside the USA, change “Printed in USA” to reflect the country in which this publication is printed.   In addition the Vendor should edit and add the “4L” CoO barcode within the page that contains “1P” part-number bar code and “07" form-number bar code and place it in between these two bar codes. CoO barcode is supplied via CoO Barcode.pdf in a .zip file. The 4L CoO conforms with IBM Engineering Spec 31L5154, Section 4.3.3.   1. The “1P” part-number barcode is included in the .PDF file. 2. The “07” form-number barcode is included in the .PDF file. | | | |