|  |  |  |
| --- | --- | --- |
| **IBM Contacts:**  **Writer:**  **EC Management:** | SPEC Owner: Juraj Kopasek (email: [jkopasek@sk.ibm.com](mailto:jkopasek@sk.ibm.com))    Backup: Sharon Norton (507) 253-2150 (email: [sharonn@us.ibm.com](mailto:sharonn@us.ibm.com))  Ryan Achilles (email: [achilles@us.ibm.com](mailto:achilles@us.ibm.com))  EC creator: jkopasek@sk.ibm.com  EC creator’s backup: [peter.holenda@sk.ibm.com](mailto:peter.holenda@sk.ibm.com) | |
| **EC Level:** | P24200 | |
| **.ZIP Package Contents:**  **ZIP File Location:**  **ISO Location:**  **Form Number** | 03KG558.doc  03KG558.cdr  03KG558.pdf  03KG558A.zip  03KG558.iso  SK5T-7087-29 | Print Instructions and Specification (this file) - Static  Media label art - Static  Representative sample of file – Static  http://public.dhe.ibm.com/systems/power/docs/hw/OMS/  https://public.dhe.ibm.com/systems/power/docs/hw/images/p10ga4/ |
| **Component:** | DVD | |
| **Print:** | 2 colors – white background w/ black text | |
| **Additional Instructions:**   1. Place media in paper sleeve with window.   **Media Labeling:** All media labels must include the text “Recorded in X” (where x is the country of origin). The full country name must be printed in English. Exception: The only country abbreviations allowed are USA and UK. This conforms to IBM Engineering Spec 31L5154. Section 4.3.3 Design (4L) CoO. Value after identifier: 2 character ISO-3166 country code. | | |