|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **IBM Contacts:**  **Writer/Requester:**  **EC Management:** | SPEC Owner: Juraj Kopasek (email: jkopasek@sk.ibm.com)     |  |  | | --- | --- | |  |  |   Backup: Sharon Norton (507) 253-2150 (email: [sharonn@us.ibm.com](mailto:sharonn@us.ibm.com))  Michal Malostik (email: [michal.malostik@sk.ibm.com](mailto:michal.malostik@sk.ibm.com))  Ryan Achilles (email: [achilles@us.ibm.com](mailto:achilles@us.ibm.com))  EC creator: [peter.holenda@sk.ibm.com](mailto:peter.holenda@sk.ibm.com)  EC creator’s backup: jkopasek@sk.ibm.com | | |
| **EC Level:** | P24145 | | |
| **.ZIP Package Contents:**  **ZIP File Location:**  **Form Number** | 03KG529.doc  03KG529.pdf  03KG529A.zip  GC43-5553-01 | | Print Instructions and Specification (this file)  Camera Ready Copy (CRC) (Covers and Body Text)  **http://public.dhe.ibm.com/systems/power/docs/hw/OMS/** |
| **Component:** | Hardcopy Manual | | |
| **Cover:** | Stock:  Color: | 80lb opaque white (or IBM approved equivalent)  2-color (black and Pantone 2718 blue) | |
| **Body Text:** | Stock:  Color:  Prints:  Page Count: | 20lb opaque white (or IBM approved equivalent)  5-color: Black, Pantone 032 Red, Pantone 108 Yellow, Pantone 2718 Blue, Pantone 1525 C Orange  2 sides (duplex)  48 | |
| **Binding:** | N/A | | |
| **Trim size:** | 8.5-in. by 11.0-in. | | |
| **Orientation:** | Portrait | | |
| **Collation:** | See the .PDF for a representative sample. | | |
| **Additional Instructions:**   1. Outside the USA, change “Printed in USA” to reflect the country in which this publication is printed.   The 4L CoO barcode conforms with IBM Engineering Spec 31L5154, Section 4.3.3.   1. The “1P” part-number barcode and “4L” Country of Origin barcode are included in the 03KG529.PDF file. | | | |