|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **IBM Contacts:**  **Writer:**  **EC Management:** | SPEC Owner: Ivona Janderlova (email: [ivona.janderlova@sk.ibm.com](mailto:ivona.janderlova@sk.ibm.com))   |  |  | | --- | --- | |  |  |   Backup: Michal Malostik (email: [michal.malostik@sk.ibm.com](mailto:michal.malostik@sk.ibm.com))  Robert Seemann (email: bseemann@us.ibm.com)  EC creator: [JGustina@sk.ibm.com](mailto:JGustina@sk.ibm.com)  EC creator’s backup: [jan.balla@sk.ibm.com](mailto:jan.balla@sk.ibm.com) | |
| **EC Level:** | P24284 | |
| **.ZIP Package Contents:**  **ZIP File Location:**  **ISO Location:**  **Form Number** | 03KG571.docx  03KG571.cdr  03KG571.pdf  03KG571B.zip  03KG571.iso  LCD8-2009-10 | Print Instructions and Specification (this file) - Static  Media label art - Static  Representative sample of file – Static  **http://public.dhe.ibm.com/systems/power/docs/hw/OMS/**  https://public.dhe.ibm.com/systems/power/docs/hw/images/p10ga5 |
| **Component:** | DVD | |
| **Print:** | 2 colors – white background w/ black text | |
| **Additional Instructions:**   1. Place media in paper sleeve with window.   **Media Labeling:** All media labels must include the text “Recorded in X” (where x is the country of origin). The full country name must be printed in English. Exception: The only country abbreviations allowed are USA and UK. This conforms to IBM Engineering Spec 31L5154. Section 4.3.3 Design (4L) CoO. Value after identifier: 2 character ISO-3166 country code. | | |